This circuit shows an inductor being driven by an AC voltage. The colors indicate power consumption; red means that a component is consuming power, and green means that the component is contributing power. The left side of the circuit represents the power company's side, and the right side represents a factory (with a large induction motor).
The highly inductive load is causing the power company to work a lot harder than normal for a given amount of power delivered. The graph on the left indicates the power lost in the power company's equipment (the resistor at top left). The graph in the middle is the power delivered to the factory. The graph on the right is the power delivered to the inductor (and then returned, causing the time average of power delivered to be zero).
Even though a peak power of 40 mW is being delivered to the factory, 200 mW is being dissipated in the power company's wires. This can happen whenever power factor is less than 1, and power companies usually charge extra when this happens.

Next: Power Factor Correction

Previous: Blocking Inductive Kickback

Index

Simulator Home

java@falstad.com
Generated Tue Oct 4 2016