This shows the frequency response of two stubs, one open and one shorted. The input source sweeps through a range of frequencies; the response is determined by the pattern of standing waves on the lines. The lower left scope shows the voltage across the terminating resistor for the open case, and the other scope shows the shorted case.

Next: Low-Pass Filter

Previous: Impedance Matching (Shunt Stub)

Index

Simulator Home

java@falstad.com
Generated Tue Oct 4 2016