This example uses four analog switches (transmission gates) to invert the input voltage. When the clock is high, the input voltage charges a capacitor. When the clock is low, the voltage across this capacitor is used to discharge another capacitor, bringing the output voltage close to the negative input voltage.

Next: Inverter Amplifier

Previous: Switchable Filter

Index

Simulator Home

java@falstad.com
Generated Tue Oct 4 2016